We are switching software to Norpix/StreamPix Lite

In this software (and Vimba Viewer) we can change camera setting. They need to be set up as follows:  
Output is LINE 3 (not Line 0). This is Line Selector in the config system


Gain = 10

Gamma = 1

Exposure: this may depend – 2.5ms

Continuous

Output on Active Frame or Active Exposure.



Exposure time 2500.005 \*can’t be right)

Gain = 10

Gamma =1

